# Fanvil

Setting up a **Fanvil** SIP phone through the phone\'s local http
management portal.

-   Factory reset the phone (physically on the phone) by pressing menu
    button \> Settings \> Advanced Settings (default password is 123) \>
    Reset to Default \> Press yes to continue.
-   Press Menu \> Status to get the phones ip address
-   Open a web browser and enter the phones ip address
-   Default login name and password is **admin**
-   Top menu click **Auto Provision**

## Common Settings

-   Fill out the fields:
    -   Authentication Name: http user name that was set in FusionPBX
        default settings
    -   Authentication Password: http password that was set in FusionPBX
        default settings
    -   Save Auto Provision Information: Check the box
    -   Download CommonConfig enabled: Check the box
    -   Download DeviceConfig enabled: Check the box

## Static Provisioning Server

-   Fill out the fields:
    -   Authentication Name: http user name that was set in FusionPBX
        default settings
    -   Server Address: <https://domain.tld/app/provision>
    -   Protocol Type: HTTPS
    -   Update Mode: Update after Reboot
-   Click Apply

![image](../../_static/images/provision/fusionpbx_provision_auto_fanvil.jpg)

-   Left side menu click **System**
-   Top menu click **Tools**
-   Scroll to the bottom and click **Reboot**

![image](../../_static/images/provision/fusionpbx_provision_auto_fanvil1.jpg)

## Self Signed Certificates

If you are going to use a self signed certificate you will need to
adjust additional settings.

-   Left side menu click **Phone settings**
-   Top menu click **Trusted Certificates**
-   CA Certificates: Disabled
-   Click Apply

![image](../../_static/images/provision/fusionpbx_provision_auto_fanvil2.jpg)
