# Polycom

## Soundpoint IP 320P

Identification

    Display Name: FusionPBX
    Address: ExtensionNumber
    Authentication User ID: ExtensionNumber
    Authentication Password: PASSWORD
    Label: ExtensionNumber or Whatever
    Type: Private
    Third Party Name: BLANK
    Number Of Line Keys: BLANK
    Calls Per Line: BLANK

Server 1

    Address: FusionBPX IP ADDRESS or DOMAIN NAME if doing multi-tenant
    Port: 5060
    Transport: DNSnaptr works or UDP or whatever
    Expires: default (30 works ok NATTED)
    Register: BLANK
    Retry Timeout: BLANK
    Retry Maximum Count: BLANK
    Line Seize Timeout: BLANK

Server 2

    leave alone

Call Diversion

    leave alone

Message Center

    Subscriber: BLANK
    Callback Mode: Contact
    Callback Contact: \*98
