Polycom
========


Soundpoint IP 320P
^^^^^^^^^^^^^^^^^^

Identification

::

    Display Name: FusionPBX
    Address: ExtensionNumber
    Authentication User ID: ExtensionNumber
    Authentication Password: PASSWORD
    Label: ExtensionNumber or Whatever
    Type: Private
    Third Party Name: BLANK
    Number Of Line Keys: BLANK
    Calls Per Line: BLANK
    
Server 1

::

    Address: FusionBPX IP ADDRESS or DOMAIN NAME if doing multi-tenant
    Port: 5060
    Transport: DNSnaptr works or UDP or whatever
    Expires: default (30 works ok NATTED)
    Register: BLANK
    Retry Timeout: BLANK
    Retry Maximum Count: BLANK
    Line Seize Timeout: BLANK

Server 2

::

    leave alone

Call Diversion

::

    leave alone

Message Center

::

    Subscriber: BLANK
    Callback Mode: Contact
    Callback Contact: \*98

