# Fanvil

Setting up a **Fanvil** SIP phone through the phone\'s local http
management portal.

-   Factory reset the phone (physically on the phone) by pressing menu
    button \> Settings \> Advanced Settings (default password is 123) \>
    Reset to Default \> Press yes to continue.
-   Press Menu \> Status to get the phones ip address
-   Open a web browser and enter the phones ip address
-   Default login name and password is **admin**
-   Left side menu click **Line**
-   Fill out the fields:
    -   Username:
    -   Display Name:
    -   Authentication Name:
    -   Authentication Password:
    -   SIP Proxy Server Address:
-   Click Apply

![image](../../_static/images/provision/fusionpbx_provision_manual_fanvil.jpg)

-   Left side menu click **System**
-   Top menu click **Tools**
-   Scroll to the bottom and click **Reboot**

![image](../../_static/images/provision/fusionpbx_provision_manual_fanvil1.jpg)
