# Yealink

Setting up a **Yealink** SIP phone through the phone\'s local http
management portal.

-   Factory reset the phone by holding down the \"OK\" button, found in
    the center of the up/down left/right buttons, until the phone
    prompts to Factory reset. Press the softkey for \"OK\" to continue.
    The phone will factory reset and reboot.
-   Once the phone powers up, press the OK button once and the phone
    will display its IP address on the screen. Navigate to that IP on
    another device in a web browser, and use admin for the username and
    admin for the password.

![image](../../_static/images/fusionpbx_t41p_login.png)

-   **Enter the following information for each Account that is
    required:**
-   Select the \"Account\" tab at the top menu.
-   Set \"Line Active\" to enabled.
-   Set \"Label\" to the user\'s name or the extension number, or both,
    ie \"John-100\".
-   Set \"Display Name\" to the same as above.
-   Set \"Register Name\" to the users FusionPBX extension number, in
    this case 100.
-   Set \"User Name\" to the users FusionPBX extension number, in this
    case 100.
-   Set \"Password\" to the users FusionPBX password.
-   If you would like to use TCP transport, set \"Trasport\" to TCP.
-   Under SIP Server 1, set the \"Server Host\" to your FusionPBX domain
    for that extension.
-   **Click confirm.**

![image](../../_static/images/fusionpbx_t41p_config.png)

-   Click \"Advanced\" on the left menu.
-   Set \"Voicemail\" to \*97
-   **Click confirm.**
