# Htek

Setting up a **Htek** SIP phone through the phone\'s local http
management portal.

-   Factory reset the phone (physically on the phone) by pressing menu
    button \> Settings \> Advanced Settings (default password is admin)
    \> Phone Settings \> Factory Reset \> Press yes to continue.
-   Press Menu \> Status \> Information to get the phones ip address
-   Open a web browser and enter the phones ip address
-   Default login name and password is **admin**
-   Top menu click **Management**
-   Left menu click **Auto Provision**
-   Fill out the following fields:
    -   Firmware Server Path:
    -   Config Server Path:
    -   HTTP/FTP/HTTPS UserName:
    -   HTTP/FTP/HTTPS Password:
-   Click **SaveSet**
-   Click **Autoprovision Now**

![image](../../_static/images/provision/fusionpbx_provision_auto_htek.jpg)

## Self Signed Certificates

Some additional settings need adjusted to provision with a self signed
certificate.

-   Top menu click **Management**

-   Left menu click **Trusted CA**

-   Choose the following

        -   Only Accept Trusted Certificates: OFF
        -   Common Name Validation: OFF
        -   Trusted Certificates: All Certificates

![image](../../_static/images/provision/fusionpbx_provision_auto_htek1.jpg)
