# Cisco

To manually provision Cisco

-   Login to the phone
-   Goto the **Ext1** top left tab
-   **Proxy and Registration** section put your servers *domain.tld* in
    the *proxy* field
-   **Subscriber Information** section put the extension number for
    *Display Name* and *User ID*
-   **Password** put the *extensions password*
-   Click **Submit All Changes** at the bottom

![image](../../_static/images/fusionpbx_provision_manual_cisco.jpg)

Once you have that done, make sure the p-time is set to 0.020

-   Click the **advanced** option at the top right
-   Goto the **SIP** tab at the top
-   Scroll down to the **RTP Parameters** section and make sure the *RTP
    Packet Size* field has *0.020*
-   Click **Submit All Changes** at the bottom

![image](../../_static/images/fusionpbx_provision_manual_cisco1.jpg)

**HTTP Authentication**

Phone web interface -\> Provision - \> Profile Rule

\[\--uid myUser \--pwd
myPass\]<http://mydomain.com/app/provision/?mac=$MA>
