# Flyingvoice

To configure the Flyingvoice phone do the following steps.

-   Once the phone powers up, press the OK button once and the phone
    will display its IP address on the screen. Navigate to that IP on
    another device in a web browser, and use admin for the username and
    admin for the password.
-   Click the **Administration** tab at the top
-   Click the **Provision** tab at the top secondary menu.
-   Under **Configuration Profile**, fill in the **Profile Rule** field.
    This will be <https://domain.tld/app/provision> Replace domain.tld
    with your actual domain name.
-   Click **Save & Apply.**

![image](../../_static/images/provision/fusionpbx_auto_flyingvoice_provision.png)
