# Parking

Call \"parking\" transfers a current call to an available park
extension, where the caller will listen to Music on Hold. The extension
that originally received the call is now free to accept other calls or
direct another extension to join the call that was parked.

For example:

:   The receptionist receives a call, and the caller would like to speak
    to the engineering department. The receptionist says \"please hold
    while I transfer you,\" and presses the PARK1 button. The call is
    sent to extension 5901 and the caller listens to music on hold. The
    receptionist is now free to make a call to her engineering staff, or
    pages the engineering page group and says \"Engineering you have a
    call on PARK1.\"

    The Engineer can press the flashing park button on his phone, and he
    will be connected to the caller, and the park extension will be
    freed for another call.

    Multiple park extensions can be created. Phones can be programmed
    with BLF functionality for parked extensions, so the users can see
    if there is a call in that extension.

Below is an example of how to provision a Yealink SIP-T32G, which has 3
Line buttons.

![image](../_static/images/call_park_yealink.jpg)
