# Htek

Setting up a **Htek** SIP phone through the phone\'s local http
management portal.

-   Factory reset the phone (physically on the phone) by pressing menu
    button \> Settings \> Advanced Settings (default password is admin)
    \> Phone Settings \> Factory Reset \> Press yes to continue.
-   Press Menu \> Status \> Information to get the phones ip address
-   Open a web browser and enter the phones ip address
-   Default login name and password is **admin**
-   Top menu click **Account**
-   Fill out the fields with **red**\* :
    -   Account Active:
    -   Primary SIP Server:
    -   SIP Transport:
    -   SIP User ID:
    -   Authenticate ID:
    -   Authenticate Password:
-   Click SaveSet
-   Click Restart

![image](../../_static/images/provision/fusionpbx_provision_manual_htek.jpg)
