INVITE sip:7271@iptel.org SIP/2.0
Via: SIP/2.0/UDP 195.37.77.99:5040
Max-Forwards: 1
From: "jiri" <sip:jiri@iptel.org>;tag=76ff7a07-c091-4192-84a0-d56e91fe104f
To: <sip:jiri@bat.iptel.org>
Call-ID: r10815e0-bf17-4afa-8412-d9130a793d96@213.20.128.35
CSeq: 2 INVITE
Contact: <sip:213.20.128.35:9315>
User-Agent: Windows RTC/1.0
Proxy-Authorization: Digest username="jiri", realm="iptel.org", algorithm="MD5", uri="sip:jiri@bat.iptel.org", nonce="3cef753900000001771328f5ae1b8b7f0d742da1feb5753c", response="53fe98db10e1074b03b3e06438bda70f"
Content-Type: application/sdp
Content-Length: 451

v=0
o=jku2 0 0 IN IP4 213.20.128.35
s=session
c=IN IP4 213.20.128.35
b=CT:1000
t=0 0
m=audio 54742 RTP/AVP 97 111 112 6 0 8 4 5 3 101
a=rtpmap:97 red/8000
a=rtpmap:111 SIREN/16000
a=fmtp:111 bitrate=16000
a=rtpmap:112 G7221/16000
a=fmtp:112 bitrate=24000
a=rtpmap:6 DVI4/16000
a=rtpmap:0 PCMU/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:4 G723/8000
a=rtpmap:5 DVI4/8000
a=rtpmap: 3 GSM/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-16
