# Yealink

To configure the Yealink phone do the following steps.

-   Login to the phone
-   Click the **Settings** tab at the top
-   On the left vertical menu click **Auto Provision**
-   Fill in the **Server URL** field. This will be
    <https://domain.tld/app/provision> Replace domain.tld with your
    actual domain name.
-   Click **Confirm** at the bottom
-   Click **Auto Provision Now** at the bottom

![image](../../_static/images/fusionpbx_provision_auto_yealink.jpg)

If you have a Certificate that is self-signed or not in the Yealink\'s
trusted certificate authority then do the following.

-   Goto the Security tab at the top right
-   On the left vertical menu click **Trusted Certificates**
-   On the dropdown box near the bottom choose **Disabled** for \"Only
    Accept Trusted Certificates\".
-   Click **Confirm**
-   The phone will reboot and then provision using the information that
    was provided.

![image](../../_static/images/fusionpbx_provision_auto_yealink1.jpg)
